Under the EU Battery Regulation (EU) 2023/1542, we must comply with new labelling laws for batteries.
Article 13 ofthis new regulation requires batteries to enter the EU with a label afixed that includes the 13 mandatory general pieces of information
根据欧盟电池法规(EU)2023/1542，我们必须遵守新的电池标签规定。
本新法规第13条规定，电池进入欧盟时必须附带包含以下13项强制性通用信息的标签:
[image: IMG_256][image: IMG_256]
1.铅或镉符号：不含铅不含镉
1.Symbol Pb or CD：This product contains no lead or cadmium. 
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2.横线垃圾桶标签：
2. Crossed-out trash can label：

3.制造商：浙江石井工具有限公司
3.Manufacturer：ZHEJIANG SHIJING TOOLS CO.,LTD

4.电池类别和识别：圆柱形可充电锂离子电池  
4. Battery category and identification：INR18650/3000mAh-3C/3.7V

5.制造地点：浙江省金华市武义县桐琴镇纬五西路1号
5.Place of manufacture：No.1, Weiwu West road, Tongqin Town, Wuyi county, Zhejiang, China

6.生产日期：2026年7月
6. Date of manufacture：July 2026

7.重量：48g
7. Weight：48g

8.化学特性：Li-ion NMC
[bookmark: _GoBack]8.Chemical characteristics：Li-ion NMC

9.危险物质的存在情况：无
9.Presence of hazardous substances：None

10.适用的灭火剂：干粉灭火器、二氧化碳灭火器
10.Suitable extinguishing agent：Dry powder fire extinguishers, Carbon dioxide fire extinguishers

11.质量占比超过0.1%的原材料：钴、锂、镍
11. Raw material exceeding 0.1% by mass：Cobalt , Lithium, Nickel

12.容量：3000mAh
12.Capacity：3000mAh


13.寿命(如非可充电)：放电容量 (500次循环) ≥80%
13. Lifetime (if non-rechargeable)：Discharge capacity (500th cycle)≥80%



自2026年8月18日起，每块电池在进入欧盟市场前必须贴上此标签。
自2027年2月18日起，每个电池表面必须印有二维码，该二维码可直接链接到13项强制性通用信息。
电池还需要CE标志和证书。欧洲电池法规第19条规定，标签必须:
1.以可见、易读且不可擦除的方式固定在电池上。若因电池特性而无法实现或无此必要，则必须将其固定
在包装上以及随电池一同提供的文件上
2.在电池投放市场或投入使用前贴附。
3.后接根据附件VII要求的公告机构识别号

Starting February 18, 2027, every individual batery must have a 0R code printed on its suriace that links directly to the 13 mandatory general pieces of
information.
The battery also needs a CE logo and certificate. Article 19 of the European Battery Regulation specifies that the label must be.
1. Affixed to the battery in a visible, legible, and indelible manner, lf this is impossible or not justified due to
the nature of the battery, it must be affixed to the packaging and to the documents accompanying the
battery
2. Affixed before the battery is placed on the market or put into service
3. Followed by the identification number of the notified body where required under Annex Vll
Can you ask Shiling ifthey already have a solution about this change in regulation? The easiest solution would be to have the OR code ready now for all
future orders.
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